
low-pass

N=1999


cutoff=350



high-pass

N=1999


cutoff=800



bandpass

N=1999

cutoff=400, 700



Echo

<https://www.youtube.com/watch?v=oe63ggMPzrY>

Q2

% Get input data wihtout normatization

% Great for bit reduction

[input, fs] = audioread('Tempest.wav', 'native');